
TTXSDK-IOS documentation




I. Preparation before integration

<https://github.com/tongtianxing/ios_cmsv6demo> , Download demo including TTXSDK.framework.zip Because github stores more than 100M files with additional strategies, the downloaded zip file size may be small.


You need to open <https://github.com/tongtianxing/ios_cmsv6demo/blob/master/TTXSDK.framework.zip> Download the more than 100 M zip files to replace the original files, or you can use the git lfs pull command to actually pull large files down after installing git lfs.

2. Integrate into your project


Import TTXSDK.framework into the project, and then ensure that "Framework Search Paths" and "User Header Search Paths" are properly configured in the "Search Path" of "Build Setting" in "TARGETS".



3. Add a dependency library



API interface


Login through the login interface of the web development interface document, and obtain vehicle information. Then configure it through TTXSDKPrepare.

Live video

Live video with TTXRealVideo instance

After the parameters are configured, the video preview is turned on, as well as the sound playback video function and so on.


Practical examples can be found in cmsv6demo



Talkback

Talkback using the TTXTalkback instance6.png

Configure the device ID of the talkback7.png

Practical examples can be found in cmsv6demo


Playback

Use TTXPlaybackSearch instance to search for playback


Callback returns an array of TTXDeviceSearchModel instances

Play playback using the TTXPlaybackView instance.

TTXPlaybackView includes playback pause adjustment progress and other functions, you can use this class to customize your own player. You can also use the player instance written by TTXPlaybackVideoController in our cmsv6demo.

Device

Device search via TTXDeviceSearch instance

Use the method to open the search, return the search result through the callback (may be empty). Search for an instance array containing TTXDeviceSearchModel. The playback device preview video is also implemented by TTXRealVideo. For the implementation process, please refer to the DeviceSearchView class of cmsv6demo.

Rights Profile

The permission configuration is configured in the project's info.plist file.

If you use the intercom function, add the corresponding configuration item in info.plist.

Privacy - Microphone Usage Description microphone

If you use video or play back screenshots and videos

Privacy - Photo Library Additions Usage Description Album

The following is the cmsv6demo sample configuration.

